
1. Click the camera icon to choose the correct camera model



6

1. Tick off

Enter correct MMS/GPRS/SMTP/FTP configuration information, phone number(s), and email account(s) into blanks;

C:\Documents and Settings\Administrator\Desktop\New Folder (3)\6.jpg

1. With all Settings entered, click **“Save**” to create MMS/GPRS configuration file “MMS.CFG”;

**Note:** MMS/GPRS configuration file will be saved into the same folder of “HuntingConfig”;

1. Copy file “MMS.CFG” into SD card; insert SD card into camera; turn on camera and enter the menu, then all settings will be saved into camera automatically.
2. If you need to change any setting information again, copy the “MMS.CFG” into

same folder of “HuntingConfig”, then click **“Load”**, thus previous setting info will be uploaded, and you can do further edition.